|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DISASTER – ELECTRICAL OUTAGE | | | | NO. | |
| 1. Call Electric Company 1-800-334-7661 2. Maintenance Supervisor is responsible to make sure electrical switches are off before electricity is restored. 3. Active alternate power supply. 4. Generator Parts: 5. “Idiot light” panel by nursing station 6. Green unit in front of ECTC     Our generator will kick on if electricity is lost to ECTC because of a power surge, storm, etc. It will do this automatically. It provides electricity for the running lights, nursing stations, exit lights, kitchen, etc.  For the residents requiring electricity for their health and safety (i.e. oxygen concentrator, suction machines) shall be assisted to an area where the generator can supply electricity. These outlets are red.  After power is restored, the engine has to “diesel-down”. This means that it will run for about 20-30 minutes after power is restored. The engine also has to test itself every so often. It will shut itself off after 20-30 minutes.  IF YOU ARE SURE THE ELECTRICITY IS ON IN THE BUILDING AND THE NOISE IS DEAFENING OR THE MACHINE IS CRANKING POORLY, YOU MAY SHUT THE UNIT OFF BY:  At the generator on the lower right hand side of the panel is a 3-position switch. It would be at the “remote mode”. Putting it in the middle will stop the generator.  Remember, if you put switch in middle, to return it to “remote” in one hour. If the machine is still on, then leave on “stop” until help arrives. | | | | | |
| Approved: | Effective Date:  3/86 | Revision Date:  2/01; 10/08; 3/17 | Change No.: | | Page:  1 of 1 |