|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| DISASTER – GAS OUTAGE | | | | NO. | |
| 1. Call Gas Company (Emergency Services) 1-800-642-6748.  2. Inform Emergency Service and Disaster Agency of problem 537-5471 or fax at 537-2388.  3. Maintenance Supervisor or designated person will be responsible to turn off gas at main valve. For location  of controls, see section entitled “Utility Controls”.  4. As a safety measure, open windows to prevent gas accumulation and possible explosion.  5. Maintenance Supervisor or other appropriate person will inspect entire Center for gas leaks  or gas accumulation and possible explosion.  6. Gas Alarm Locations:  a. Boiler room  b. Back laundry  c. Kitchen  d. Independence Way  Continuously monitor indoor air for natural gas for leaks to prevent potentially explosive or asphyxial conditions.  7. If residents have to be evacuated, see section entitled “Evacuation of Residents”.  8. REMEMBER: WHEN GAS IS RESTORED, PILOT LIGHTS ON GAS SUPPLIED EQUIPMENT MUST BE RELIT. | | | | | |
| Approved: | Effective  Date: | Revision  Date:  3/17 | Change No.: | | Page:  1 of 1 |