**Maintained Log Bed & Side Rail Safety Check**

Resident Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Room Number:\_\_\_\_\_\_\_

Resident Height:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Resident Weight:\_\_\_\_\_\_\_\_\_\_\_\_\_

 Date Date Date Date Date

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| The distance between slats is no more than 4.5 inches. |  |  |  |  |  |
| Bed Rails are mechanically sound firmly attached, latches are in working order. |  |  |  |  |  |
| Space between rail & mattress and mattress & head/footboard as no more than 2.5 inches. |  |  |  |  |  |
| Longest distance of triangular space at the head of the bed is no more than 4.5 inches. |  |  |  |  |  |

Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_